page1
<
>
COLLEGA
SCOLLEGA
Start Hz
start MHz.
Stop Hz
stop  MHz.
Punti
points
SCANSIONE
STOP
Punti acquisiti
acquired
SHORT
LOAD
ISOL
THRU
CAL DONE
SALVA CAL
CARICA CAL
OPEN
 
CONNECT
DISCONNECT
SCAN
EXIT
continue
COM
slow
acquired in
msec.
CAL APPLY
SAVE CAL
LOAD CAL
S11
S21
RLC
PHASE
ROS
???
RLC limits     
1 pF to 1 uF
10 nHe to 10 mHe
at freq.
MHz.
SMD probe
R.O.S.
S11 phase
S11 mag
S21 phase
S21 db
RE
IM
ok
FASE
GAIN
RLC bridge                                        
SMD Test
